Hello Marlin

I enjoyed talking with you.

I learned about a new TNC, Thanks

Kenwood TM-281 cable to wire up to a 6 pin mini din female.

To hookup to Mobilinkd Bluetooth APRS TNC 6 pin mini din male cable

**( 4 wire cable w/shield )**

**White** - MIC - goes to **PIN 1 mini din**

**Red** - PTT - goes to **PIN 3 mini din**

**grounds and shields** between the two cables

are soldered together and go to **PIN 2 of mini din**

I usually solder ground last and cut to size then.

I found the smallest diameter 1/8" cable I could find

**( 2 wire cable with 1/8 " plug )**

White - RECEIVE AUDIO -  goes to **PIN 5 of mini din for 1200 baud TNC**

OR

White - RECEIVE AUDIO -  goes to **PIN 4 of mini din for 9600 baud TNC**

I will print this and put with cable.

Les - WY0GTR

[www.jivetones.com/hamparts](http://www.jivetones.com/hamparts)

[wy0gtr@jivetones.com](mailto:wy0gtr@jivetones.com)

[wy0gtr@winlink.org](mailto:wy0gtr@winlink.org)

913-749-6367 cell/text